(module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 55B68D4A)
  (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
  (tags "SPST Button Switch")
  (fp_text reference SW1 (at -0.1 -0.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value RESET (at -7.7 2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 1.75 -0.05) (layer F.SilkS) (width 0.15))
  (fp_line (start 5.05 3.4) (end 5.05 -3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.05 -3.4) (end -5.05 3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.05 3.4) (end 5.05 3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -5.05 -3.4) (end 5.05 -3.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.225 -3.225) (end 3.225 -3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.225 3.225) (end 3.225 3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.225 3.225) (end -3.225 3.1) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.225 -3.1) (end -3.225 -3.225) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.225 -1.4) (end 3.225 1.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.225 -3.225) (end 3.225 -3.225) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.225 -1.4) (end -3.225 1.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.225 3.225) (end 3.225 3.225) (layer F.SilkS) (width 0.15))
  (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask))
)
