(module SRR1210 (layer F.Cu) (tedit 54D2B1D8)
  (fp_text reference L201 (at 4.225 8.275) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 1mH (at 64.95 -93.3) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -6 -6) (end 6 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 -6) (end 6 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 6) (end -6 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 6) (end -6 -6) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at 0 5.05) (size 5.3 2.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 -5.05) (size 5.3 2.8) (layers F.Cu F.Paste F.Mask))
)
