(module project_foot:W3113-OffsetPad (layer F.Cu) (tedit 55B7C4FF)
  (fp_text reference P3 (at -0.8 0.6) (layer F.SilkS) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_text value P102 (at 0 -12) (layer F.Fab) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start 0 0) (end 4 0) (layer F.SilkS) (width 0.3))
  (fp_line (start -6.25 0) (end -6.25 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start -6.25 -8) (end -4 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start 6.25 0) (end 6.25 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start 6.25 -8) (end 4 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start 6 0) (end 6.25 0) (layer F.SilkS) (width 0.25))
  (fp_line (start -6 0) (end -6.25 0) (layer F.SilkS) (width 0.25))
  (fp_line (start -4 0) (end -6 0) (layer F.SilkS) (width 0.25))
  (fp_line (start 4 0) (end 6 0) (layer F.SilkS) (width 0.25))
  (fp_line (start -4 -1) (end -4 0) (layer F.SilkS) (width 0.25))
  (fp_line (start -4 0) (end 0 0) (layer F.SilkS) (width 0.25))
  (fp_line (start 1 0) (end 1 -1) (layer F.SilkS) (width 0.25))
  (fp_line (start 1 -1) (end 5 -1) (layer F.SilkS) (width 0.25))
  (fp_line (start 4 -1) (end 4 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start 4 -8) (end 0 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start 0 -8) (end -4 -8) (layer F.SilkS) (width 0.25))
  (fp_line (start -4 -8) (end -4 -1) (layer F.SilkS) (width 0.25))
  (pad "" np_thru_hole circle (at -4 0) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 1 smd rect (at 2 -0.5) (size 4 1) (drill (offset 1 0)) (layers F.Cu F.Paste F.Mask))
  (pad "" np_thru_hole circle (at 5.2 -2.1) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  (pad "" np_thru_hole circle (at -5.25 -7) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
)
