(module w_project:crystal_smd_5x3.2mm (layer F.Cu) (tedit 55DF6EA9)
  (descr "5x3.2mm SMD glass Crystal")
  (fp_text reference X301 (at 0 -2) (layer F.SilkS)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_text value 32.768Mhz (at 0 2.1) (layer F.SilkS) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start -1.8 -0.8) (end 1.8 -0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.8 -0.7) (end 1.8 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.8 0.8) (end -1.8 0.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 0.8) (end -1.8 -0.7) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -1.2 0) (size 1.1 1.9) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.06858))
  (pad 2 smd rect (at 1.2 0) (size 1.1 1.9) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.06858))
  (model walter/crystal/crystal_smd_5x3.2mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
