(module project_footprints:Motor_Pololu_Encoder (layer F.Cu) (tedit 57277F47)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference P12 (at -6 6.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MOTOR_B (at -6 -7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 24.5 -2) (end 36.5 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 36.5 -2) (end 36.5 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 36.5 1.5) (end 24.5 1.5) (layer F.SilkS) (width 0.15))
  (fp_arc (start 21.1 -8) (end 17.6 -8) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 21 -8) (end 21 -11.5) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 21 8) (end 24.5 8) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_arc (start 20.9 8) (end 20.9 11.5) (angle 90) (layer F.SilkS) (width 0.15))
  (fp_line (start 24.5 -6) (end 24.5 -8) (layer F.SilkS) (width 0.15))
  (fp_line (start 24.5 -8) (end 14.5 -8) (layer F.SilkS) (width 0.15))
  (fp_line (start 14.5 -8) (end 14.5 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 14 6) (end 14 8) (layer F.SilkS) (width 0.15))
  (fp_line (start 14 8) (end 24.5 8) (layer F.SilkS) (width 0.15))
  (fp_line (start 24.5 8) (end 24.5 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 4) (end -5.5 4) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.5 4) (end -5.5 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start -5.5 -4) (end -2.5 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5 -4) (end -2 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -6) (end 24.5 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 24.5 -6) (end 24.5 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 24.5 6) (end -2 6) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 6) (end -2 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 -3.73) (end -1.27 -3.73) (layer F.SilkS) (width 0.15))
  (pad 0 thru_hole circle (at 21 9) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (pad 1 smd rect (at -0.25 -5) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.25 -3) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.25 -1) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -0.25 1) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.25 3) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -0.25 5) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
  (pad 0 thru_hole circle (at 21 -9) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
    (at (xyz 0 -0.25 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
