(module CR-1220_HFN (layer F.Cu) (tedit 5466129F)
  (fp_text reference CR-1220_HFN (at 3.6 4) (layer F.SilkS) hide
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_text value VAL** (at 10 -3) (layer F.SilkS)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_circle (center 3 0) (end 3 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4 -1) (end 4 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 4 1) (end 7 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 1) (end 7 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -1) (end 4 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 -2) (end 10 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 10 2) (end -2 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 2) (end -2 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -2 -2) (end 10 -2) (layer F.SilkS) (width 0.15))
  (fp_circle (center 3 0) (end -3 0) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 10 0) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS))
)
