(module Pin_Headers:Pin_Header_Angled_1x02 (layer F.Cu) (tedit 566850A9)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference P3 (at 0 -5.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.7 -1.5) (end 2.8 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.7 -0.9) (end 4.7 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 -0.9) (end 4.7 -0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 -1.5) (end 2.8 -0.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 0.7) (end 2.8 1.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.8 1.3) (end 4.7 1.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.7 1.3) (end 4.7 0.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.7 0.7) (end 2.8 0.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 -2) (end -1.8 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 -2) (end -1.2 -1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.2 -1.8) (end -1.2 1.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.2 1.7) (end -1.5 2) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.5 2) (end 1 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.8 -2) (end 8 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 -2) (end 8 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 8 2) (end 6.8 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.8 2) (end 6.8 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.8 1.5) (end 6.3 1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.3 -1.5) (end 6.8 -1.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.8 -1.5) (end 6.8 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 2) (end 6.3 2) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.3 2) (end 6.3 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 6.3 -2) (end 1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 2) (end 1 -2) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.25 -2) (end -1.25 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.25 -2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -2) (end 6.25 -2) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 2) (end 6.25 2) (layer F.CrtYd) (width 0.05))
  (pad 1 thru_hole rect (at 0 -1) (size 1.25 1.25) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 0 1) (size 1.25 1.25) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02.wrl
    (at (xyz 0 -0.05 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
