(module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5667CDF3)
  (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
  (tags "capacitor 0402")
  (attr smd)
  (fp_text reference REF** (at 0 -2.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value I_1212 (at 0 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2 -1.9) (end 1.9 -1.9) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.9 -1.9) (end 1.9 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.9 1.8) (end -1.8 1.8) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.8 1.8) (end -1.8 -1.9) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at 1.1 0) (size 1.15 3.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.1 0) (size 1.15 3.3) (layers F.Cu F.Paste F.Mask))
  (model Capacitors_SMD.3dshapes/C_0402.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
