(module TO_SOT_Packages_SMD:TSOT-6-MK06A_Handsoldering (layer F.Cu) (tedit 56B619B7)
  (descr "TSOP-6 MK06A housing 6pin")
  (attr smd)
  (fp_text reference U2 (at -0.07112 -4.35102) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USBLC6-2 (at -0.03048 5.22986) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center -1.1 0.5) (end -0.9 0.6) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.7 -0.5) (end -0.7 0.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.7 0.5) (end 0.7 0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.7 0.4) (end 0.7 -0.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.7 -0.5) (end -0.7 -0.5) (layer F.SilkS) (width 0.15))
  (pad 1 smd rect (at -0.5 0.8) (size 0.3 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 0.8) (size 0.3 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.5 0.8) (size 0.3 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.5 -0.8) (size 0.3 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0 -0.8) (size 0.3 0.99) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -0.5 -0.8) (size 0.3 0.99) (layers F.Cu F.Paste F.Mask))
  (model TO_SOT_Packages_SMD.3dshapes/TSOT-6-MK06A_Handsoldering.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
