(module PULSE_ETH_TRANS (layer F.Cu) (tedit 54D7CCDF)
  (fp_text reference PULSE_ETH_TRANS (at 0 -8) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_text value VAL** (at 0 9) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_line (start -0.75 -2.5) (end -0.75 -0.25) (layer F.SilkS) (width 0.25))
  (fp_line (start -0.75 -0.25) (end -0.75 0) (layer F.SilkS) (width 0.25))
  (fp_line (start -1 -2.5) (end -0.5 -2.5) (layer F.SilkS) (width 0.25))
  (fp_line (start -0.5 -2.5) (end -0.5 0) (layer F.SilkS) (width 0.25))
  (fp_line (start -1 0) (end 10 0) (layer F.SilkS) (width 0.25))
  (fp_line (start 10 0) (end 10 -8.5) (layer F.SilkS) (width 0.25))
  (fp_line (start 10 -8.5) (end -1 -8.5) (layer F.SilkS) (width 0.25))
  (fp_line (start -1 -8.5) (end -1 0) (layer F.SilkS) (width 0.25))
  (pad 1 smd rect (at 0 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.27 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.54 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 3.81 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 5.08 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 6.35 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 7.62 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 8.89 0) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 8.89 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 7.62 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 6.35 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 5.08 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 3.81 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 2.54 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 1.27 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 0 -8.51) (size 0.76 1.65) (layers F.Cu F.Paste F.Mask))
)
