(module Oddities:NetTie-I_Connected_SMD placed (layer F.Cu) (tedit 5509E5A3)
  (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
  (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
  (fp_text reference JP1002 (at 0.35 1.65) (layer F.SilkS)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_text value JUMPER (at 0.25 -2.15 270) (layer F.Fab) hide
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start 1.778 -1.016) (end -1.778 -1.016) (layer F.Cu) (width 0.3048))
  (fp_line (start -1.778 -0.762) (end 1.778 -0.762) (layer F.Cu) (width 0.3048))
  (fp_line (start 1.778 -0.508) (end -1.778 -0.508) (layer F.Cu) (width 0.3048))
  (fp_line (start -1.778 -0.254) (end 1.778 -0.254) (layer F.Cu) (width 0.3048))
  (fp_line (start 1.778 0) (end -1.778 0) (layer F.Cu) (width 0.3048))
  (fp_line (start -1.778 0.254) (end 1.778 0.254) (layer F.Cu) (width 0.3048))
  (fp_line (start 1.778 0.508) (end -1.778 0.508) (layer F.Cu) (width 0.3048))
  (fp_line (start -1.778 0.762) (end 1.778 0.762) (layer F.Cu) (width 0.3048))
  (fp_line (start 1.778 1.016) (end -1.778 1.016) (layer F.Cu) (width 0.3048))
  (pad 1 smd rect (at -2.54 0) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 2.54 0) (size 1.99898 1.99898) (layers F.Cu F.Paste F.Mask))
)
