(module Battery_3xAAA_Holder (layer F.Cu) (tedit 56E1D285)
  (fp_text reference REF** (at 0 3.3) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Battery_3xAAA_Holder (at -10.5 -27.7) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -19 26.3) (end 19 26.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 19 26.3) (end 19 -26.3) (layer F.SilkS) (width 0.15))
  (fp_line (start 19 -26.3) (end -19 -26.3) (layer F.SilkS) (width 0.15))
  (fp_line (start -19 -26.3) (end -19 26.3) (layer F.SilkS) (width 0.15))
  (pad 0 thru_hole circle (at 12.7 0) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at 0 -23.72) (size 2 2) (drill 1) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 12.7 -23.72) (size 2 2) (drill 1.02) (layers *.Cu *.Mask F.SilkS))
  (pad 0 thru_hole circle (at -12.7 0) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask F.SilkS))
)
