(module "OS102011MS2QN1 Slide Switch" (layer F.Cu)
  (fp_text reference "OS102011MS2QN1 Slide Switch" (at 0 -3.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value VAL** (at 0 3.4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 4.3 -2.1) (end 4.3 -1.5) (layer F.SilkS) (width 0.25))
  (fp_line (start 4.3 2.1) (end 4.3 1.5) (layer F.SilkS) (width 0.25))
  (fp_line (start -4.3 1.6) (end -4.3 1.5) (layer F.SilkS) (width 0.25))
  (fp_line (start -4.3 2.1) (end -4.3 1.6) (layer F.SilkS) (width 0.25))
  (fp_line (start -4.3 -2.1) (end -4.3 -1.5) (layer F.SilkS) (width 0.25))
  (fp_line (start 4.3 2.15) (end -4.3 2.15) (layer F.SilkS) (width 0.25))
  (fp_line (start -4.3 -2.15) (end 4.3 -2.15) (layer F.SilkS) (width 0.25))
  (pad "" thru_hole circle (at 4.1 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad "" thru_hole circle (at -4.1 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at -2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
)
