(module CDRH127 (layer F.Cu) (tedit 54D7CB7A)
  (fp_text reference CDRH127 (at 0 -6) (layer F.SilkS) hide
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_text value VAL** (at -2 6) (layer F.SilkS)
    (effects (font (size 0.5 0.5) (thickness 0.125)))
  )
  (fp_line (start -4 5) (end 4 5) (layer F.SilkS) (width 0.25))
  (fp_line (start -6 3) (end -6 -3) (layer F.SilkS) (width 0.25))
  (fp_line (start 6 -3) (end 6 3) (layer F.SilkS) (width 0.25))
  (fp_line (start -4 -5) (end 4 -5) (layer F.SilkS) (width 0.25))
  (fp_text user R.M.S. (at 0 0) (layer F.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.15)))
  )
  (fp_arc (start 4 3) (end 6 3) (angle 90) (layer F.SilkS) (width 0.25))
  (fp_arc (start -4 3) (end -4 5) (angle 90) (layer F.SilkS) (width 0.25))
  (fp_arc (start -4 -3) (end -6 -3) (angle 90) (layer F.SilkS) (width 0.25))
  (fp_arc (start 4 -3) (end 4 -5) (angle 90) (layer F.SilkS) (width 0.25))
  (pad 1 smd rect (at 0 -4.95) (size 5.4 2.9) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 4.95) (size 5.4 2.9) (layers F.Cu F.Paste F.Mask))
)
