(module project_footprints:BARREL_JACK_065center (layer F.Cu) (tedit 56AF818E)
  (descr "DC Barrel Jack")
  (tags "Power Jack")
  (fp_text reference CON1 (at 10.09904 0 90) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BARREL_JACK (at 1.2004 -3.301) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 2 2.5) (end 2 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 -1) (end 12 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start 12 -1) (end 12 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 12 1) (end 11 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 2.5) (end 0 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -2.5) (end 11 -2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 -2.5) (end 11 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 2.5) (end 0 2.5) (layer F.SilkS) (width 0.15))
  (pad 0 thru_hole circle (at 3 0 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
  (pad 1 smd rect (at 12 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 10 -3.75) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 9 3.75) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask))
  (pad 0 thru_hole circle (at 8.5 0 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
)
