(module project_footprints:SonarSensor_HCSR04 (layer F.Cu) (tedit 570407E8)
  (descr "Through hole pin header")
  (tags "pin header")
  (fp_text reference P16 (at -6.2 -5.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SONAR_1 (at -3 5.27 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 12.4 -5.6) (end 15 -5.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 -5.6) (end 15 5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 15 5.2) (end 12.4 5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.2 20.8) (end 26 20.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 26 20.8) (end 26 8.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 26 8.8) (end 12.2 8.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.2 -20.2) (end 26 -20.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 26 -20.2) (end 26 -9.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 26 -9.2) (end 12.4 -9.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.2 22.4) (end 12.2 -22.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.2 -22.4) (end 11 -22.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 -22.4) (end 11 22.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 11 22.4) (end 12.2 22.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.8 -5.6) (end 10.4 -5.6) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.4 -5.6) (end 10.4 5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.4 5.2) (end 1.4 5.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.4 5.2) (end 1.4 5) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.75 -5.75) (end -1.75 5.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.75 -5.75) (end 1.75 5.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 -5.75) (end 1.75 -5.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.75 5.4) (end 1.75 5.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.27 -2.73) (end -1.27 4.89) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 -2.73) (end 1.27 4.89) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.55 -5.55) (end 1.55 -4) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 4.89) (end 1.27 4.89) (layer F.SilkS) (width 0.15))
  (fp_line (start 1.27 -2.73) (end -1.27 -2.73) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.55 -4) (end -1.55 -5.55) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.55 -5.55) (end 1.55 -5.55) (layer F.SilkS) (width 0.15))
  (pad 4 thru_hole rect (at 0 -3.81) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole oval (at 0 -1.27) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole oval (at 0 1.27) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole oval (at 0 3.81) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
  (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
    (at (xyz 0 -0.15 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
