(module Connect:SD_Card_Receptacle (layer F.Cu) (tedit 5708027E)
  (fp_text reference REF** (at 1.4 -2.35) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MicroSD_Card_Receptacle (at 3.55 3.3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.45 0.05) (end 10.55 0.05) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.55 0.05) (end 10.55 -10.55) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.55 -10.55) (end -1.3 -10.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.3 -10.5) (end -1.3 0.05) (layer F.SilkS) (width 0.15))
  (pad 9 smd rect (at -1.3 -7.75) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 10.25 -0.15) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 7.7 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 6.6 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 5.5 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 4.4 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 3.3 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.2 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.1 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 0 0) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.4 -0.15) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 10.55 -8.4) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask))
)
